

**Northern Chamber of Information Technology**

**Tel: 021 221 6629**

**Email:** [**chaiman@ncit.lk**](mailto:chaiman@ncit.lk)

**Web : www. ncit.lk**

**136C, Parameswara Junction,**

**Palaly Road, Thirunelvely,**

**Jaffna, Sri Lanka.**

Northern Chamber of Information Technology,

Jaffna.

26.05.2018

……………………………………….

……………………………………….

……………………………………….

.……………………………..

**QUOTATION FOR SUPPLY OF MULTIMEDIA PROJECTOR**

Herewith we are furnishing our quotation for supply of **multimedia projector** to the Northern Chamber of Information Technology , Jaffna.

|  |  |
| --- | --- |
| Item | Multimedia Projector |
| No of Items | 01 |
| Specification | Annexed |

Quotations are addressed to:

Chairman,

Northern Chamber of Information Technology,

136C, Parameswara Junction,

Palaly Road, Thirunelvely, Jaffna, Sri Lanka.

Quotation No: NCIT/2018/06

Closing Date of Quotation: 31.05.2018

Chairman,

Northern Chamber of Information Technology, Jaffna

……………………………………….

………………………………………

………………………………………

.………………………………………

Chairman,

Northern Chamber of Information Technology,

136C, Parameswara Junction,

Palaly Road, Thirunelvely, Jaffna, Sri Lanka.

**QUOTATION FOR SUPPLY OF MULTIMEDIA PROJECTOR**

Quotation for supply of **multimedia projector** to the Northern Chamber of Information Technology , Jaffna.

|  |  |
| --- | --- |
| Item | Multimedia Projector |
| No of Items | 01 |
| Specification | Annexed |
| Price with vat |  |

Validity of quotation: Months

....................................................................

Manager Signature

Quotation No: NCIT/2018/06

Closing Date of Quotation: 31.05.2018

**Technical Specification & Compliance**

**Item Name: Multimedia Projector**

**No of Items: 01**

|  |  |  |  |
| --- | --- | --- | --- |
| **Specification** | **Minimum requirements** | **Bidders response** | |
| **Compliance**  **(Yes / No)** | **If “No” Comment(s) on the Offer** |
| Make | Specify |  |  |
| Model | Specify |  |  |
| Country of Origin | Specify |  |  |
| Country of Manufacture | Specify |  |  |
| Projection System | 3LCD, 3-chip technology TFT Active matrix |  |  |
| Projection Method | Front /rear / ceiling mount |  |  |
| Pixel Number | 480,000 dots (800×600)×3 |  |  |
| Colour Brightness | 2600 lumens |  |  |
| White Brightness | 2600 lumens |  |  |
| Aspect Ratio | 4:3 |  |  |
| Native Resolution | 800×600 (SVGA) |  |  |
| Lamp Life | Normal mode: Up to 2000 hours |  |  |
| Projected distance | 3' to 10' |  |  |
| Keystone Correction | Vertical/ Horizontal ±30 degrees |  |  |
| USB Plug 'n Play | Projector is compatible with PC and Mac® computers |  |  |
| Contrast Ratio | Up to 3000:1 |  |  |
| Colour Reproduction | 16.77 million colours |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Projection Lens | F-number: 1.44  Focal Length: 16.7 mm  Zoom Ratio: Optical zoom 1.0 – 1.35 |  |  |
| Input Signal | NTSC /NTSC4.43/PAL/M-PAL/N-PAL/PAL60/SECAM/SDTV/HDTV |  |  |
| Operating Angle: | Right / Left: ±30 degrees  Upper / Lower: ±15 degrees |  |  |
| Interfaces | * Computer / Component video: D-sub 15 pin x 1 * S-video: Mini DIN x 1 * Composite video: RCA (Yellow) x 1 * Audio in: Stereo Mini x 1 * USB connector: Type B x 1 * Monitor out: D-sub 15 pin x 1 * Audio out: Stereo Mini x 1 * Serial : RS-232c x1 * RJ45 |  |  |
| Power Supply Voltage: | 100–230 V±10%, 50/60Hz |  |  |
| Dimensions | Specify |  |  |
| Weight | Specify |  |  |
| Others | Remote Control |  |  |
| Warranty | Two Years (Comprehensive) |  |  |