

**Northern Chamber of Information Technology**

**Tel: 021 221 6629**

**Email:** [**chaiman@ncit.lk**](mailto:chaiman@ncit.lk)

**Web : www. ncit.lk**

**136C, Parameswara Junction,**

**Palaly Road, Thirunelvely,**

**Jaffna, Sri Lanka.**

Northern Chamber of Information Technology,

Jaffna.

26.05.2018

……………………………………….

……………………………………….

……………………………………….

.……………………………..

**QUOTATION FOR SUPPLY PROJECTOR CEILING MOUNT**

Herewith we are furnishing our quotation for supply of **Projector Ceiling Mount** to the Northern Chamber of Information Technology Business Incubation Centre training hall , Jaffna.

|  |  |
| --- | --- |
| Item | Projector Ceiling Mount |
| No of Items | 01 |
| Specification | Annexed |

Quotations are addressed to:

Chairman,

Northern Chamber of Information Technology,

136C, Parameswara Junction,

Palaly Road, Thirunelvely, Jaffna, Sri Lanka.

Quotation No: NCIT/2018/08

Closing Date of Quotation: 31.05.2018

Chairman,

Northern Chamber of Information Technology, Jaffna

**Specification of Projector Ceiling Mount**

**Specification:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Specification** | **Minimum requirements** | **Bidders response** | |
| **Compliance**  **(Yes / No)** | **If “No” Comment(s) on the Offer** |
| Type | variable height |  |  |
| Projector to ceiling gap (min) | 15.4 inches (390 mm) |  |  |
| Projector to ceiling gap (max) | 23.8 inches (605 mm) |  |  |
| Maximum projector weight | 25 lbs. (11.4 kg) |  |  |
| Maximum pan angle | 360° |  |  |
| Maximum tilt angle | 30° down / 30° up |  |  |
| Maximum roll angle | 30° left / 30° right |  |  |
| Materials and finish | White powder coated aluminium and steel |  |  |
| Net product weight | Specify |  |  |
| Unit Price | Specify |  |  |

Note: Please give your compliance Yes/No, If No please give your comments on the offer